#N canvas 4 52 570 713 10;
#X obj 96 51 gemreceive;
#X text 169 51 ordered receive;
#X obj 72 227 gemreceive foo -1;
#X obj 72 249 print first;
#X obj 412 227 gemreceive foo 12;
#X obj 412 249 print third;
#X obj 282 227 gemreceive foo 1996;
#X obj 282 249 print fourth;
#X obj 182 249 print second;
#X obj 72 196 s foo;
#X text 58 91 [gemreceive] takes an additional argument (compared to
Pd's [receive]) that specifies the priority.;
#X text 61 136 The higher the number \, the later the object will receive!
;
#X obj 182 227 gemreceive foo;
#X text 223 169 the default priority is "0";
#X text 76 298 1st inlet allows you to change the receiver name;
#X obj 107 371 gemreceive bar;
#X obj 107 393 print foobar;
#X msg 235 337 FOO;
#X msg 273 337 BAR;
#X obj 273 359 s bar;
#X msg 123 351 symbol bar;
#X text 80 443 2nd inlet let's you change the priority on the fly;
#X obj 116 610 gemreceive foobar 10;
#X obj 252 610 gemreceive foobar 20;
#X obj 116 632 print left;
#X obj 252 632 print right;
#X msg 116 464 left2right;
#X obj 116 518 t a a;
#X obj 233 520 route left2right right2left;
#X msg 202 464 right2left;
#X msg 233 542 10 20;
#X msg 312 543 20 10;
#X obj 233 564 unpack;
#X obj 116 540 s foobar;
#X msg 72 173 bang;
#X obj 235 359 s fou;
#X msg 107 331 symbol fou;
#X connect 2 0 3 0;
#X connect 4 0 5 0;
#X connect 6 0 7 0;
#X connect 12 0 8 0;
#X connect 15 0 16 0;
#X connect 17 0 35 0;
#X connect 18 0 19 0;
#X connect 20 0 15 0;
#X connect 22 0 24 0;
#X connect 23 0 25 0;
#X connect 26 0 27 0;
#X connect 27 0 33 0;
#X connect 27 1 28 0;
#X connect 28 0 30 0;
#X connect 28 1 31 0;
#X connect 29 0 27 0;
#X connect 30 0 32 0;
#X connect 31 0 32 0;
#X connect 32 0 22 1;
#X connect 32 1 23 1;
#X connect 34 0 9 0;
#X connect 36 0 15 0;
