#N canvas 5 31 889 373 12;
#X graph graph1 0 1 100 -1 67 250 267 350;
#X array array99 100 float;
#X pop;
#X obj 29 181 metro 500;
#X obj 13 126 phasor~;
#X floatatom 13 76 0 0 0;
#X obj 57 12 phasor~;
#X obj 29 156 r metro;
#X obj 13 100 sig~ 890;
#X text 78 75 <-- specify frequency;
#X text 92 98 <-- convert it to audio signal;
#X msg 409 75 \; metro 0;
#X msg 405 18 \; pd dsp 1 \; metro 1;
#X text 494 32 <-- Click to start;
#X text 479 79 <-- Click to stop;
#X text 129 14 - sawtooth generator;
#X text 170 207 <-- graph the output;
#X text 82 128 <-- right inlet resets phase;
#X obj 425 227 phasor~ 440;
#X floatatom 425 203 0 0 0;
#X text 348 118 The phasor~ object outputs a sawtooth signal \, traditionally used for table lookup via cos~ or tabread4~. If no argument is supplied \, the input is taken to be an audio signal \; with a floating-point argument \, phasor~ takes floating-point messages to change frequency.;
#X text 294 246 Invoked above with argument for non-signal input. Incoming messages override the initial value.;
#X text 311 301 see also:;
#X obj 396 301 osc~;
#X obj 439 301 cos~;
#X obj 481 301 tabread4~;
#X text 627 345 updated for Pd version 0.33;
#X obj 13 205 tabwrite~ array99;
#X connect 1 0 25 0;
#X connect 2 0 25 0;
#X connect 3 0 6 0;
#X connect 5 0 1 0;
#X connect 5 0 1 0;
#X connect 6 0 2 0;
#X connect 17 0 16 0;
