#N canvas -4 364 603 514 10;
#X obj 145 292 f;
#X obj 175 292 + 1;
#X obj 46 160 t b b;
#X msg 161 268 0;
#X obj 125 355 sel 1;
#X msg 48 218 0;
#X msg 46 191 1;
#X floatatom 452 292 7 0 0 0 - - -;
#X obj 442 333 phasor~;
#X obj 415 384 cos~;
#X obj 450 384 cos~;
#X obj 449 361 -~ 0.25;
#X obj 46 134 inlet;
#X obj 394 413 outlet~;
#X obj 451 413 outlet~;
#X obj 216 329 t f f;
#X obj 217 391 outlet;
#X msg 114 122 \; pd dsp 1;
#X obj 125 332 >= \$1;
#X msg 498 333 0;
#X obj 145 237 metro;
#X text 166 7 filter-graph1 -- generate sinusoids to test a filter
;
#X text 168 23 arg 1: number of steps - arg2: frequency range;
#X text 40 53 This \, together with its companion filter-graph2 \,
measure a filter's frequency and phase response. Here we count from
0 to n-1 (where n is the table size) and output the index and a complex
sinusoid at each frequency to test.;
#X text 222 192 fudge to estimate settling time;
#X obj 487 67 loadbang;
#X obj 487 105 t b b;
#X obj 519 151 max 1;
#X obj 487 128 f \$2;
#X obj 519 128 f \$1;
#X obj 487 151 /;
#X obj 442 265 *;
#X obj 217 367 pack;
#X floatatom 500 183 5 0 0 0 - - -;
#X floatatom 248 237 5 0 0 0 - - -;
#X obj 487 86 bng 15 250 50 0 empty empty empty 0 -6 0 8 -262144 -1
-1;
#X obj 202 173 expr max(50 \, 40000/($f2*max($f1 \, 1)));
#X connect 0 0 1 0;
#X connect 0 0 15 0;
#X connect 0 0 18 0;
#X connect 1 0 0 1;
#X connect 2 0 6 0;
#X connect 2 1 3 0;
#X connect 2 1 17 0;
#X connect 3 0 0 1;
#X connect 4 0 5 0;
#X connect 5 0 20 0;
#X connect 6 0 20 0;
#X connect 8 0 11 0;
#X connect 8 0 9 0;
#X connect 9 0 13 0;
#X connect 10 0 14 0;
#X connect 11 0 10 0;
#X connect 12 0 2 0;
#X connect 15 0 32 0;
#X connect 15 1 31 0;
#X connect 15 1 36 0;
#X connect 18 0 4 0;
#X connect 19 0 8 1;
#X connect 20 0 0 0;
#X connect 20 0 19 0;
#X connect 25 0 35 0;
#X connect 26 0 28 0;
#X connect 26 1 29 0;
#X connect 27 0 30 1;
#X connect 28 0 30 0;
#X connect 29 0 27 0;
#X connect 30 0 31 1;
#X connect 30 0 33 0;
#X connect 30 0 36 1;
#X connect 31 0 7 0;
#X connect 31 0 8 0;
#X connect 31 0 32 1;
#X connect 32 0 16 0;
#X connect 35 0 26 0;
#X connect 36 0 20 1;
#X connect 36 0 34 0;
#X connect 36 0 32 1;
