#N canvas 533 67 651 393 12;
#X obj 124 11 bp~;
#X text 159 11 - BANDPASS FILTER;
#X obj 70 263 env~;
#X floatatom 70 283 0 0 0;
#X floatatom 104 193 0 0 0;
#X obj 12 261 env~;
#X floatatom 12 282 0 0 0;
#X text 119 264 env~ gives the amplitude of the signal envelop in dB.
;
#X floatatom 12 123 0 0 0;
#X msg 544 67 \; pd dsp 0;
#X obj 12 146 osc~ 100;
#X text 57 121 <-- scroll to change input frequency;
#X msg 72 170 clear;
#X text 122 169 <-- reinitialize internal state;
#X text 398 361 updated for Pd version-0.30;
#X msg 544 28 \; pd dsp 1;
#X text 13 73 The left inlet is the incoming audio signal \, the middle
control input sets center frequency and the rigth input sets "Q".;
#X text 136 194 <-- center frequency;
#X obj 72 241 bp~ 100 10;
#X text 169 242 Arguments initialize center frequency and Q.;
#X text 12 301 Compare the amplitude of the original signal on the
left with the amplitude of the filtered signal on the right.;
#X floatatom 153 215 0 0 0;
#X text 185 216 <-- Q;
#X text 16 35 bp~ passes a sinusoid at the center frequency at unit
gain (approximately). Other frequencies are attenuated.;
#X text 21 357 see also:;
#X obj 110 356 vcf~;
#X connect 2 0 3 0;
#X connect 4 0 18 1;
#X connect 5 0 6 0;
#X connect 8 0 10 0;
#X connect 10 0 5 0;
#X connect 10 0 18 0;
#X connect 12 0 18 0;
#X connect 18 0 2 0;
#X connect 21 0 18 2;
