#N canvas 191 0 534 413 10;
#X obj 21 14 pow~;
#X obj 67 109 sig~;
#X obj 98 173 loadbang;
#X obj 98 197 metro 100;
#X obj 98 221 snapshot~;
#X floatatom 67 73 5 0 0 0 - - -;
#X obj 108 109 sig~;
#X floatatom 108 73 5 0 0 0 - - -;
#X obj 68 138 pow~ 2;
#X floatatom 98 246 7 0 0 0 - - -;
#X obj 413 268 pow~ 2;
#X text 20 271 An optional creation argument initializes right inlet:
;
#X text 319 384 updated for Pd version 0.42.;
#X text 23 303 WARNING: it's easy to generate "infinity" by accident
\, and if you do \, the DSP chain may dramatically slow down if you're
using an i386 or ia64 processor. Out-of-range floating point values
are thousands of times slower to compute with than in-range ones.;
#X text 68 12 - raise a signal to a numeric power (given by another
signal). The left inlet must be a positive number. The right inlet
my be positive \, zero \, or negative.;
#X connect 1 0 8 0;
#X connect 2 0 3 0;
#X connect 3 0 4 0;
#X connect 4 0 9 0;
#X connect 5 0 1 0;
#X connect 6 0 8 1;
#X connect 7 0 6 0;
#X connect 8 0 4 0;
