# This is a qlist for patch number 68, which demonstrates an oscillator

bank.

;

# comments start with a "#" which must be followed by a space.  The comment

is terminated by a semicolon like this: ;



# first an arpeggio.  You can group them in lines as you please.  The 100s at

the beginnings of lines are delay times. ;



pit1 89; amp1 80;

100 pit2 72; amp2 80;

100 pit3 57; amp3 90;

100 pit4 84; amp4 78;

100 pit5 74; amp5 74;

100 pit6 73; amp6 74;

100 pit7 100; amp7 78;

100 pit8 37; amp8 95;



# after a 600-msec rest, gliss four of the oscillators to new frequencies. ;

600 pit1 70 1000;

300 pit8 40 1000;

300 pit4 89 1000;

300 pit7 95 1000;



# a second later, turn them off with decay time 1500 ;

1000

amp1 0 1500;

amp2 0 1500;

amp3 0 1500;

amp4 0 1500;

amp5 0 1500;

amp6 0 1500;

amp7 0 1500;

amp8 0 1500;



# and re-attack them.. ;

1000

amp1 85 5;

amp2 85 5;

amp3 85 5;

amp4 90 5;

amp5 85 5;

amp6 85 5;

amp7 90 5;

amp8 85 5;



# this time, try varying decay times. ;

10

amp1 0 2000;

amp2 0 2000;

amp3 0 2000;

amp4 0 500;

amp5 0 1000;

amp6 0 1000;

amp7 0 500;

amp8 0 4000;

