#N canvas 518 85 518 450 12;
#X obj 36 168 clip~ -0.5 0.5;
#X obj 58 252 metro 500;
#X obj 12 16 clip~;
#X text 171 137 inlets to reset clip range;
#X floatatom 83 137 5 -1 1 0 - - - 0;
#X text 146 169 creation arguments initialize clip range;
#X text 11 412 see also:;
#X obj 91 413 clip;
#X obj 176 413 min~;
#X obj 130 413 expr~;
#X msg 153 244 \; pd dsp \$1;
#X obj 58 227 loadbang;
#N canvas 629 138 568 290 reference 0;
#X obj 8 48 cnv 5 550 5 empty empty INLETS: 8 18 0 13 #202020 #000000 0;
#X obj 8 79 cnv 1 550 1 empty empty 1st: 8 12 0 13 #9f9f9f #000000 0;
#X obj 8 166 cnv 2 550 2 empty empty OUTLET: 8 12 0 13 #202020 #000000 0;
#X obj 8 203 cnv 2 550 2 empty empty ARGUMENTS: 8 12 0 13 #202020 #000000 0;
#X obj 8 108 cnv 1 550 1 empty empty 2nd: 8 12 0 13 #7c7c7c #000000 0;
#X obj 8 137 cnv 1 550 1 empty empty 3rd: 8 12 0 13 #7c7c7c #000000 0;
#X text 153 112 float - set lower limit., f 49;
#X text 153 140 float - set upper limit., f 49;
#X obj 31 16 clip~;
#X obj 7 260 cnv 5 550 5 empty empty empty 8 18 0 13 #202020 #000000 0;
#X text 133 213 1) float - initial lower limit (default 0)., f 49;
#X text 133 232 2) float - initial upper limit (default 0)., f 49;
#X text 78 16 - restrict signal(s) between two limits.;
#X text 145 84 signal(s) - signal value(s) to clip., f 50;
#X text 145 176 signal(s) - the clipped signal(s)., f 49;
#X restore 350 14 pd reference;
#X text 441 13 <= click;
#X obj 4 47 cnv 1 505 1 empty empty empty 8 12 0 13 #000000 #000000 0;
#X text 56 15 - restrict a signal between two limits;
#X obj 36 294 tabwrite~ clip;
#X floatatom 131 138 5 -1 1 0 - - - 0;
#X text 80 114 lower;
#X text 130 114 upper;
#X obj 4 400 cnv 1 505 1 empty empty empty 8 12 0 13 #000000 #000000 0;
#X text 133 61 The [clip~] object passes its signal input to its output \, clipping it to lie between two limits., f 50;
#X obj 290 225 cnv 19 198 98 empty empty empty 20 12 0 12 #ffffff #404040 0;
#N canvas 0 22 450 278 (subpatch) 0;
#X array clip 200 float 0;
#X coords 0 1 199 -1 200 100 1 0 0;
#X restore 289 224 graph;
#X obj 36 72 osc~ 500;
#X obj 153 208 set-dsp-tgl;
#X text 184 212 DSP on/off;
#N canvas 741 60 410 608 multichannel 0;
#X text 59 25 [clip~] works with multichannel signals \, where the operation is performed in all existing channels., f 41;
#X obj 72 135 snake~ in, f 10;
#X obj 72 243 snake~ out;
#X obj 171 332 snapshot~;
#X floatatom 171 371 6 0 0 0 - - - 0;
#X obj 72 332 snapshot~;
#X floatatom 72 371 6 0 0 0 - - - 0;
#X msg 240 179 \; pd dsp \$1;
#X text 272 142 DSP on/off;
#X obj 240 138 set-dsp-tgl;
#X obj 72 200 clip~ -0.5 0.5;
#X obj 72 405 vsl 19 162 -1 1 0 0 empty empty empty 0 -9 0 12 #dfdfdf #000000 #000000 0 1;
#X obj 171 405 vsl 19 162 -1 1 0 0 empty empty empty 0 -9 0 12 #dfdfdf #000000 #000000 0 1;
#X obj 171 265 metro 150;
#X obj 171 236 loadbang;
#X obj 72 105 osc~ 0.5;
#X obj 139 105 osc~ 0.25;
#X connect 1 0 10 0;
#X connect 2 0 5 0;
#X connect 2 1 3 0;
#X connect 3 0 4 0;
#X connect 4 0 12 0;
#X connect 5 0 6 0;
#X connect 6 0 11 0;
#X connect 9 0 7 0;
#X connect 10 0 2 0;
#X connect 13 0 3 0;
#X connect 13 0 5 0;
#X connect 14 0 13 0;
#X connect 15 0 1 0;
#X connect 16 0 1 1;
#X restore 273 356 pd multichannel;
#X text 122 341 mutichannel signal support ----------->, f 20;
#X text 298 412 updated for Pd version 0.54;
#X obj 216 413 wrap~;
#X connect 0 0 16 0;
#X connect 1 0 16 0;
#X connect 4 0 0 1;
#X connect 11 0 1 0;
#X connect 17 0 0 2;
#X connect 24 0 0 0;
#X connect 25 0 10 0;
