#N canvas 512 61 490 403 12;
#X obj 90 280 snapshot~;
#X floatatom 90 314 6 0 0 0 - - - 0;
#X obj 27 13 sig~;
#X obj 90 151 sig~;
#X floatatom 90 119 6 0 0 0 - - - 0;
#X obj 112 226 metro 200;
#X text 266 366 updated for Pd version 0.33;
#X text 140 119 <= Scroll to set value, f 12;
#X obj 112 195 loadbang;
#X text 353 126 DSP on/off;
#X obj 206 240 sig~ 10;
#X obj 206 280 snapshot~;
#X floatatom 206 206 6 0 0 0 - - - 0;
#X floatatom 206 314 6 0 0 0 - - - 0;
#X text 271 232 An argument initializes the signal value., f 23;
#X msg 319 157 \; pd dsp \$1;
#X text 14 366 see also:;
#X obj 90 365 snapshot~;
#X obj 7 43 cnv 1 475 1 empty empty empty 8 12 0 13 #000000 #000000 0;
#X obj 6 351 cnv 1 475 1 empty empty empty 8 12 0 13 #000000 #000000 0;
#N canvas 667 102 424 185 reference 0;
#X obj 8 45 cnv 5 400 5 empty empty INLET: 8 18 0 13 #202020 #000000 0;
#X obj 8 87 cnv 2 400 2 empty empty OUTLET: 8 12 0 13 #202020 #000000 0;
#X obj 7 152 cnv 5 400 5 empty empty empty 8 18 0 13 #202020 #000000 0;
#X obj 8 116 cnv 2 400 2 empty empty ARGUMENT: 8 12 0 13 #202020 #000000 0;
#X obj 31 13 sig~;
#X text 67 13 - convert numbers to signals;
#X text 109 58 float - number to convert to signal.;
#X text 102 93 signal - converted signal.;
#X text 104 123 1) float - initially convertedd value.;
#X restore 315 14 pd reference;
#X text 409 14 <= click;
#X text 63 13 - convert numbers to signals;
#X text 47 57 [sig~] object converts numbers to an audio signal. In this example \, the [snapshot~] converts back again., f 53;
#X obj 319 120 set-dsp-tgl;
#X connect 0 0 1 0;
#X connect 3 0 0 0;
#X connect 4 0 3 0;
#X connect 5 0 0 0;
#X connect 5 0 11 0;
#X connect 8 0 5 0;
#X connect 10 0 11 0;
#X connect 11 0 13 0;
#X connect 12 0 10 0;
#X connect 24 0 15 0;
