#N canvas 486 26 596 595 12;
#X declare -stdpath ./;
#X obj 72 512 output~;
#X text 352 533 updated for Pd version 0.39;
#X obj 151 454 metro 250;
#X obj 151 427 tgl 19 0 empty empty empty 0 -6 0 8 #dfdfdf #000000 #000000 0 1;
#X text 174 426 graphing on/off;
#N canvas 0 0 450 300 (subpatch) 0;
#X array H02-graph 882 float 0;
#X coords 0 1 881 -1 200 140 1 0 0;
#X restore 371 311 graph;
#X text 415 456 --- 0.02 sec ---;
#X text 36 41 Many synthesis algorithms and transformations can have outputs with a zero-frequency component (commonly called DC for "direct current"). These are inaudible and sometimes cause distortion in audio output devices \, or when converting to fixed-point soundfile formats. It is often desirable to filter an audio signal to remove its DC component., f 65;
#X text 36 137 The simplest way to do this is to use a one-pole low-pass filter \, tuned to a low frequency such as 3 Hertz \, and to subtract its output from the original. This difference is called a one-pole \, one-zero high-pass filter \, and it is used so often that Pd provides one in the "hip~" object., f 65;
#X obj 71 263 +~ 1;
#X obj 71 400 hip~ 5;
#X text 134 400 high-pass filter;
#X floatatom 110 364 5 0 0 0 - - - 0;
#X msg 110 289 0;
#X text 155 238 sinusoidal test signal;
#X text 117 263 add "DC";
#X text 148 289 zero for no filtering;
#X msg 120 312 3;
#X text 155 313 3 (or so) to remove DC;
#X text 160 337 higher frequencies affect;
#X text 202 351 the audible part of;
#X text 202 367 the signal as well.;
#X obj 71 238 osc~ 220;
#X msg 128 337 220;
#X text 102 9 ONE-POLE \, ONE-ZERO HIGH-PASS FILTER;
#X obj 133 480 tabwrite~ H02-graph;
#X obj 425 8 declare -stdpath ./;
#X connect 2 0 25 0;
#X connect 3 0 2 0;
#X connect 9 0 10 0;
#X connect 10 0 0 0;
#X connect 10 0 25 0;
#X connect 12 0 10 1;
#X connect 13 0 12 0;
#X connect 17 0 12 0;
#X connect 22 0 9 0;
#X connect 23 0 12 0;
