#N canvas 505 23 564 697 12;
#X obj 47 361 rpole~;
#X obj 68 441 cpole~;
#X obj 92 472 cpole~;
#X obj 68 409 *~;
#X msg 476 469 clear;
#X obj 133 194 loadbang;
#X obj 141 536 rzero~;
#X obj 171 598 czero~;
#X obj 197 634 czero~;
#X obj 171 566 /~;
#X obj 385 350 tgl 15 0 empty empty empty 0 -6 0 8 #fcfcfc #000000
#000000 0 50;
#X obj 47 332 *~;
#X obj 141 508 /~;
#X obj 161 229 samplerate~;
#X obj 161 255 / 2;
#X obj 115 283 / 22050;
#X obj 115 230 f \$1;
#X obj 115 256 t f b;
#X obj 115 162 inlet;
#X obj 396 196 loadbang;
#X obj 385 162 inlet;
#X obj 261 194 loadbang;
#X obj 297 231 samplerate~;
#X obj 297 257 / 2;
#X obj 251 285 / 22050;
#X obj 251 257 t f b;
#X obj 251 162 inlet;
#X obj 47 162 inlet~;
#X obj 476 162 inlet;
#X obj 197 662 outlet~;
#X obj 251 232 f \$2;
#X obj 385 234 f \$3;
#X text 47 141 audio;
#X text 107 140 lp freq;
#X text 229 140 hp freq;
#X text 362 142 hi/lo norm;
#X text 477 139 clear;
#X text 24 11 3-pole \, 3-zero butterworth lp/hp/shelving filter. Args:
lp freq \, hp freq \, normalize-hi. Inlets: input signal \, lo freq
\, hi freq \, hi norm \, reset., f 74;
#X text 24 66 For high-pass: set LP freq =0 and hi/lo to 1, f 74;
#X text 24 45 For low-pass: set HP freq >= SR/2 and hi/lo to 0, f
74;
#X text 24 88 Shelving: HP and LP specify shelving band. Gain difference
is about HP/LP cubed (so HP=2LP should give about 18 dB \, for example.)
, f 74;
#X obj 115 315 buttercoef3;
#X obj 208 491 buttercoef3;
#X connect 0 0 3 0;
#X connect 1 0 2 0;
#X connect 1 1 2 1;
#X connect 2 0 12 0;
#X connect 3 0 1 0;
#X connect 4 0 0 0;
#X connect 4 0 1 0;
#X connect 4 0 2 0;
#X connect 4 0 6 0;
#X connect 4 0 7 0;
#X connect 4 0 8 0;
#X connect 5 0 16 0;
#X connect 6 0 9 0;
#X connect 7 0 8 0;
#X connect 7 1 8 1;
#X connect 8 0 29 0;
#X connect 9 0 7 0;
#X connect 10 0 41 1;
#X connect 10 0 42 1;
#X connect 11 0 0 0;
#X connect 12 0 6 0;
#X connect 13 0 14 0;
#X connect 14 0 15 1;
#X connect 15 0 41 0;
#X connect 16 0 17 0;
#X connect 17 0 15 0;
#X connect 17 1 13 0;
#X connect 18 0 16 0;
#X connect 19 0 31 0;
#X connect 20 0 31 0;
#X connect 21 0 30 0;
#X connect 22 0 23 0;
#X connect 23 0 24 1;
#X connect 24 0 42 0;
#X connect 25 0 24 0;
#X connect 25 1 22 0;
#X connect 26 0 30 0;
#X connect 27 0 11 0;
#X connect 28 0 4 0;
#X connect 30 0 25 0;
#X connect 31 0 10 0;
#X connect 41 0 11 1;
#X connect 41 1 3 1;
#X connect 41 2 0 1;
#X connect 41 3 1 2;
#X connect 41 3 2 2;
#X connect 41 4 1 3;
#X connect 41 5 2 3;
#X connect 42 0 12 1;
#X connect 42 1 9 1;
#X connect 42 2 6 1;
#X connect 42 3 7 2;
#X connect 42 3 8 2;
#X connect 42 4 7 3;
#X connect 42 5 8 3;
