#N canvas 569 23 555 685 12;
#X floatatom 68 557 6 0 0 0 - - - 0;
#X floatatom 322 310 5 0 999 0 - \$0-osc2 - 12;
#X obj 322 334 osc~;
#X text 39 14 ENVELOPE FOLLOWER;
#X text 32 41 An envelope follower measures the mean square power of an signal as it changes over time. (You can convert mean square power to RMS amplitude or to decibels if you wish.) The term "mean square" means simply that the signal should be squared \, and then averaged. The averaging is done using a low-pass filter such as lop~., f 70;
#X obj 248 491 lop~;
#X floatatom 273 462 4 0 100 0 - \$0-lop - 0;
#X obj 247 366 +~;
#X obj 247 335 osc~ 500;
#X obj 248 428 *~;
#X obj 248 554 snapshot~;
#X floatatom 248 611 7 0 999 0 - - - 0;
#X obj 248 584 sqrt;
#X obj 68 584 dbtorms;
#X floatatom 68 611 5 0 999 0 - - - 0;
#N canvas 536 459 382 265 startup 0;
#X obj 44 18 loadbang;
#X obj 44 42 bng 19 250 50 0 empty empty empty 0 -6 0 8 #dfdfdf #000000 #000000;
#X obj 44 71 f \$0;
#X text 57 199 This subpatch loads initial;
#X text 60 217 values in number boxes.;
#X obj 245 136 metro 250;
#X obj 245 111 r \$0-metro;
#X obj 245 160 s \$0-tick;
#X msg 44 95 \; \$1-osc2 400 \; \$1-lop 10 \; \$1-metro 1;
#X connect 0 0 1 0;
#X connect 1 0 2 0;
#X connect 2 0 8 0;
#X connect 5 0 7 0;
#X connect 6 0 5 0;
#X restore 78 361 pd startup;
#X text 301 429 square the signal;
#X text 336 523 take snapshot;
#X text 294 583 convert to RMS;
#X text 308 652 updated for Pd version 0.39;
#X text 293 491 low-pass filter;
#X text 309 610 output;
#X obj 259 526 r \$0-tick;
#X text 336 539 every 1/4 second;
#X obj 68 411 r \$0-tick;
#X obj 68 532 f;
#X obj 86 490 env~;
#X text 33 216 The env~ object at right \, which is a built-in envelope follower using a higher-quality low-pass filter than lop~ \, is shown for comparison. Its output is artificially slowed down to match the homemade one at left., f 70;
#X obj 322 388 *~;
#X obj 340 363 tgl 19 0 empty empty empty 0 -6 0 8 #dfdfdf #000000 #000000 0 1;
#X text 32 122 Here we're adding two oscillators so the result should be an RMS of one if the second oscillator is on \, 0.707 otherwise. Note two effects: first \, the more responsive the envelope follower \, the less accurate the result (but the faster it responds). Second \, if the two oscillators are tuned close to each other their beating affects the numbers coming out., f 70;
#X text 365 363 <= on/off;
#X text 129 512 built-in envelope follower for comparison, f 12;
#X text 308 462 <= responsiveness;
#X text 83 308 frequency of second oscillator =>;
#X obj 402 276 ../5.reference/set-dsp-tgl;
#X text 433 279 DSP on/off;
#X msg 402 313 \; pd dsp \$1;
#X connect 0 0 13 0;
#X connect 1 0 2 0;
#X connect 2 0 28 0;
#X connect 5 0 10 0;
#X connect 6 0 5 1;
#X connect 7 0 9 0;
#X connect 7 0 9 1;
#X connect 7 0 26 0;
#X connect 8 0 7 0;
#X connect 9 0 5 0;
#X connect 10 0 12 0;
#X connect 12 0 11 0;
#X connect 13 0 14 0;
#X connect 22 0 10 0;
#X connect 24 0 25 0;
#X connect 25 0 0 0;
#X connect 26 0 25 1;
#X connect 28 0 7 1;
#X connect 29 0 28 1;
#X connect 35 0 37 0;
