#N canvas 565 104 485 393 12;
#X obj 31 17 spigot;
#X text 88 16 - pass or block messages;
#X msg 93 141 0.5 1000;
#X obj 110 307 print;
#X msg 120 197 walk the cat;
#X text 173 227 control: nonzero to pass messages \, zero to stop them, f 28;
#X text 260 362 updated for Pd version 0.38;
#X obj 149 234 tgl 19 0 empty empty empty 0 -6 0 8 #dfdfdf #000000 #000000 0 1;
#X text 164 274 optional arg sets the initial state (0 by default), f 29;
#X obj 110 274 spigot;
#X obj 12 49 cnv 1 460 1 empty empty empty 8 12 0 13 #000000 #000000 0;
#X text 390 16 <= click;
#N canvas 707 220 571 252 reference 0;
#X obj 8 52 cnv 5 550 5 empty empty INLET: 8 18 0 13 #202020 #000000 0;
#X obj 8 145 cnv 2 550 2 empty empty OUTLET: 8 12 0 13 #202020 #000000 0;
#X obj 7 219 cnv 5 550 5 empty empty empty 8 18 0 13 #202020 #000000 0;
#X obj 8 182 cnv 2 550 2 empty empty ARGUMENT: 8 12 0 13 #202020 #000000 0;
#X obj 7 114 cnv 1 550 1 empty empty 2nd: 8 12 0 13 #7c7c7c #000000 0;
#X obj 9 83 cnv 1 550 1 empty empty 1st: 8 12 0 13 #7c7c7c #000000 0;
#X obj 31 17 spigot;
#X text 88 16 - pass or block messages;
#X text 142 121 float - nonzero to pass messages \, zero to stop them.;
#X text 120 88 anything - any message to pass or not., f 55;
#X text 123 192 1) float - initialize right inlet., f 52;
#X text 122 155 anything - any input message if spigot is opened.;
#X restore 296 16 pd reference;
#X obj 12 349 cnv 1 460 1 empty empty empty 8 12 0 13 #000000 #000000 0;
#X text 24 59 [spigot] passes messages from its left inlet to its outlet \, as long as a nonzero number is sent to its right inlet. When its right inlet gets zero \, incoming messages are "blocked" i.e. \, ignored.;
#X obj 110 169 bng 19 250 50 0 empty empty empty 17 7 0 10 #dfdfdf #000000 #000000;
#X connect 2 0 9 0;
#X connect 4 0 9 0;
#X connect 7 0 9 1;
#X connect 9 0 3 0;
#X connect 15 0 9 0;
