#N canvas 30 68 949 754 12;
#X obj 67 77 osc~ 440;
#X obj 67 329 dac~;
#X obj 67 242 *~;
#X obj 86 180 line~;
#X text 116 330 <-- out;
#X text 124 9 LINES GRAPHED;
#X text 24 33 Here again is a line~ controlling the amplitude of an
osc~ \, but with the outputs graphed:;
#X obj 149 89 r graphit;
#X obj 151 179 r graphit;
#X obj 151 246 r graphit;
#X obj 86 149 r to-line;
#X graph graph1 0 -1.02 44100 1.02 631 480 831 350;
#X array product 44100 float 0;
#X pop;
#X graph graph1 0 -1.02 44100 1.02 631 150 831 20;
#X array osc-output 44100 float 0;
#X pop;
#X graph graph1 0 -1.02 44100 1.02 631 315 831 185;
#X array line-output 44100 float 0;
#X pop;
#X obj 149 119 tabwrite~ osc-output;
#X obj 67 299 *~ 0.1;
#X msg 38 401 \; pd dsp 1 \; to-line 0 \, 1 500 \; graphit bang;
#X msg 210 401 \; pd dsp 1 \; to-line 1 \, 0 500 \; graphit bang;
#X obj 151 209 tabwrite~ line-output;
#X obj 151 276 tabwrite~ product;
#X text 70 379 ramp up;
#X text 235 378 ramp down;
#X text 406 376 to 1/2;
#X msg 375 400 \; pd dsp 1 \; to-line 0.5 1000 \; graphit bang;
#X text 634 491 ------ 1 second ------;
#X text 38 485 Click the message boxes above to try it. Note that in
the first two boxes \, the line~ objects get two messages. The first
one \, with no time value \, causes the line~ to jump immediately to
the value. The third box takes line~'s previous value as a point of
departure. What you see will depend on which box you last clicked and
how long you waited between the two.;
#X text 662 727 updated for Pd version 0.33;
#X text 41 600 On most machines \, you will hear an interruption in
the sound one second after you click on the first or third box. This
is because the graphical updates are likely to eat more CPU time than
your audio buffer has pre-buffered for. You can avoid this if you keep
your graphs in sub-windows and open them only when you need them. In
some future version of Pd this behavior will be improved. Until then
\, you'll have to avoid having arrays getting re-drawn during music
performances.;
#X connect 0 0 2 0;
#X connect 0 0 14 0;
#X connect 2 0 15 0;
#X connect 2 0 19 0;
#X connect 3 0 2 1;
#X connect 3 0 18 0;
#X connect 7 0 14 0;
#X connect 8 0 18 0;
#X connect 9 0 19 0;
#X connect 10 0 3 0;
#X connect 15 0 1 0;
