#N canvas 649 71 500 361 12;
#X obj 126 267 snapshot~;
#X obj 151 237 phasor~ 1;
#X floatatom 126 298 10 0 0 0 - - - 16;
#X text 25 18 CONVERTING SIGNALS TO CONTROLS;
#X text 276 299 Updated for Pd version 0.37;
#X obj 126 201 metro 100;
#X obj 126 168 tgl 19 0 empty empty empty 17 7 0 10 #dfdfdf #000000 #000000 0 1;
#X text 31 51 The [snapshot~] object allows you to convert from signals to control streams (float messages) -- an opposite of [sig~]. The value output is always the end of the most recently computed audio block \, so that even if you bang it metronomically (as here) it need not give you samples that are exactly evenly spaced., f 62;
#X obj 280 165 ../5.reference/set-dsp-tgl;
#X text 311 168 DSP on/off;
#X msg 280 202 \; pd dsp \$1;
#X connect 0 0 2 0;
#X connect 1 0 0 0;
#X connect 5 0 0 0;
#X connect 6 0 5 0;
#X connect 8 0 10 0;
