#N canvas 259 41 994 546 12;
#X obj 456 358 qlist;
#X msg 476 140 rewind;
#X msg 482 165 next;
#X floatatom 456 461 5 0 0 0 - - - 0;
#X obj 488 417 print done;
#X msg 467 114 tempo 1;
#X text 13 303 To run it manually \, send "rewind" followed by "next". All messages not preceded by numbers are sent. As soon as a message starting with one or more numbers is encountered \, the numbers are output as a list. There are many ways you could design a sequencer around this., f 56;
#X text 479 88 sequence automatically;
#X text 526 113 set relative tempo;
#X text 526 141 go to beginning (and stop);
#X text 518 164 single-step forward;
#X text 615 291 read a file;
#X text 666 314 write one;
#X text 509 454 This outlet gets a list of leading numbers for the next message \, for you to use in designing your own sequencer.;
#X msg 508 291 read qlist.txt;
#X msg 514 314 write /tmp/qlist.txt;
#X text 17 512 see also:;
#X obj 90 513 textfile;
#X msg 494 217 clear;
#X msg 499 244 add 500 this is another message;
#X msg 504 268 add2 that;
#X text 540 217 empty the qlist;
#X text 725 245 add a message to a qlist;
#X text 577 267 add a message to a qlist but don't terminate it;
#X text 576 401 This outlet gets a bang when you hit the end of the sequence. In the file "qlist.txt" the end is delayed 1000 milliseconds after the last message., f 49;
#X text 713 64 These receives are invoked in the file "qlist.txt" in this directory., f 35;
#X obj 44 14 qlist;
#X text 97 13 - text-based sequencer;
#X text 541 190 single-step forward SUPPRESSING MESSAGE-SENDING;
#X msg 488 191 next 1;
#X msg 446 63 print;
#X text 492 62 print contents to Pd window;
#X obj 488 389 bng 19 250 50 0 empty empty empty 17 7 0 10 #dfdfdf #000000 #000000;
#X obj 161 513 text sequence;
#X obj 754 110 r this;
#X obj 847 110 r that;
#X obj 847 139 print that;
#X obj 754 139 print this;
#X obj 9 45 cnv 1 975 1 empty empty empty 8 12 0 13 #000000 #000000 0;
#N canvas 751 121 568 419 reference 0;
#X obj 8 42 cnv 5 550 5 empty empty INLET: 8 18 0 13 #202020 #000000 0;
#X obj 8 260 cnv 2 550 2 empty empty OUTLETS: 8 12 0 13 #202020 #000000 0;
#X obj 8 356 cnv 2 550 2 empty empty ARGUMENTS: 8 12 0 13 #202020 #000000 0;
#X obj 7 392 cnv 5 550 5 empty empty empty 8 18 0 13 #202020 #000000 0;
#X obj 7 319 cnv 1 550 1 empty empty 2nd: 8 12 0 13 #7c7c7c #000000 0;
#X obj 7 285 cnv 1 550 1 empty empty 1st: 8 12 0 13 #7c7c7c #000000 0;
#X obj 26 9 qlist;
#X text 79 8 - text-based sequencer;
#X text 112 52 bang - start sequence automatically., f 61;
#X text 49 71 tempo <float> - set relative tempo., f 70;
#X text 98 90 rewind - go to beginning (and stop)., f 63;
#X text 48 108 next <float> -;
#X text 161 108 single-step forward \, optional floar suppresses message sending., f 54;
#X text 105 140 print - print contents to Pd window., f 62;
#X text 105 158 clear - empty the qlist., f 62;
#X text 42 176 add <anything> - add a message to a qlist., f 71;
#X text 35 195 add2 <anything> - add a message to a qlist but don't terminate it., f 72;
#X text 49 214 read <symbol> - read a file into qlist., f 70;
#X text 42 233 write <symbol> - write contents to a file., f 71;
#X text 107 291 list - list of leading numbers for the next message.;
#X text 107 324 bang - when reaching the end of sequence.;
#X text 140 366 NONE;
#X restore 807 14 pd reference;
#X text 901 14 <= click;
#X obj 9 501 cnv 1 975 1 empty empty empty 8 12 0 13 #000000 #000000 0;
#X text 530 356 click to see its contents and edit it \, just like a "text define" object., f 38;
#X text 764 512 Updated for Pd version 0.35;
#X text 503 356 <--;
#X obj 456 88 bng 19 250 50 0 empty empty empty 17 7 0 10 #dfdfdf #000000 #000000;
#X text 14 69 The [qlist] object reads text files containing time-tagged Pd messages. You can have them sequenced automatically (by sending a "bang" message \, possibly changing speed via "tempo" messages) or manually via the "rewind" and "next" messages.;
#X text 13 153 To run the qlist automatically \, send it a "read" message (the filename is relative to the directory the patch is in) and later a "bang." Messages in the file are separated by semicolons. Optional leading numbers are delay times in milliseconds. If the tempo is different from 1 the messages are sent faster or slower accordingly. Messages should start with a symbol giving the destination object. In the file "qlist.txt" used here \, the messages go to objects "this" and "that" which are receives below., f 56;
#X text 14 385 You can also record textual messages and save them to a file. Send "clear" to empty the [qlist] and "add" to add messages (terminated with semicolons.) The message \, "add2" adds a list of atoms without finishing with a semicolon in case you want to make variable-length messages., f 56;
#X text 263 512 <-- newer and better replacement for [qlist];
#X connect 0 0 3 0;
#X connect 0 1 32 0;
#X connect 1 0 0 0;
#X connect 2 0 0 0;
#X connect 5 0 0 0;
#X connect 14 0 0 0;
#X connect 15 0 0 0;
#X connect 18 0 0 0;
#X connect 19 0 0 0;
#X connect 20 0 0 0;
#X connect 29 0 0 0;
#X connect 30 0 0 0;
#X connect 32 0 4 0;
#X connect 34 0 37 0;
#X connect 35 0 36 0;
#X connect 45 0 0 0;
